TR0116 Production report instruction (i1Profiler on Mac)

1. Go to: "http://www.fredkuo.idv.tw/PSAproduction3/" to download the TDF.

2. Open i1Profiler and click [Measure Reference Chart].
 ¬

3. Click [Load Workflow] and open the TDF (ControlTarget20TDF_et.rwxf)¬

4. After open the TDF, start the batch reading for 20 production strips.
¬

5. Click "Save" when the reading is done.
¬

6. Save the data as "i1Profiler CGATS Spectral (*.txt)"
¬

7.  Go to "http://www.fredkuo.idv.tw/PSAproduction3/" to upload the data.

8. Submit the data and get the production report.